DEGREE OF HAZARDS

The low and high hazard classifications shall be required to install a backflow prevention device.

Applications requiring backflow prevention devices shall include, but shall not be limited to the following:

Low Hazard:

* Water Softeners and other treatment systems
* Restaurants
* Fountains
* Fire Line Systems
* Docks on Lakes, Rivers, Ponds, etc.…
* Automatic Water Systems for Animals

High Hazard:

* Hospitals, Doctor/Dental Offices, Medical Facilities, etc...
* High-Rise Buildings
* Wells
* Car Washes
* Hotels/Motels
* Beauty Salons
* RV Parks/Campgrounds
* Water Plants
* Industry with toxic chemicals
* Irrigation Systems
* Veterinaries, Animal Clinics, Kennels, Grooming Facilities, Zoos, Animal Refuges, etc.…
* Wastewater Treatment Plants, Lift Stations, etc.…